In ROS:

In order to write a publisher in which you send a KEY or any command from your keyboard and it will Subscribed in controller and displayed on LCD or on terminal then this code will help you.

Basically in Arduino IDE I write a generic publisher and you burn code in an Arduino controller anyone and can send values/keys/commands from your PC keyboard and can easily perform accordingly.